16-25 Principal Economic and Technical Indicators of National Railway Transport
Item | 2002 | 2003 | 2004 | 2005 | 2006
Average Daily Ton-kilometers of Freight | 102.2 | 105.8 | 108.7 | 110.6 | 114.3
Locomotives (10 000 ton-km) |  |  |  |  |
Diesel Locomotives | 99.3 | 101.4 | 103.4 | 105.6 | 108.5
Electric Locomotives | 106.8 | 112.8 | 117.1 | 118.3 | 122.7
Average Total Tonnage of Freight Locomotives (ton) | 2789 | 2829 | 2934 | 3038 | 3105
Diesel Locomotives | 2648 | 2679 | 2768 | 2848 | 2887
Electric Locomotives | 3028 | 3071 | 3198 | 3335 | 3425
Daily Distance per Freight Locomotive (km) | 445 | 450 | 455 | 458 | 465
Daily Distance per Passenger Locomotive (km) | 557 | 562 | 612 | 650 | 671
Oil Consumption of Diesel Locomotives | 25.9 | 25.4 | 25.0 | 24.6 | 24.3
(kg/10 000 ton-km) |  |  |  |  |
Electricity Consumption of Electric Locomotives | 110.8 | 110.0 | 111.2 | 111.8 | 110.0
(kwh/10 000 ton-km) |  |  |  |  |
Punctuality Rate of Freight Trains at Departure (%) | 97.3 | 96.9 | 96.5 | 97.0 | 97.4
Punctuality Rate of Freight Trains in Running (%) | 96.7 | 96.5 | 96.2 | 96.9 | 97.3
Punctuality Rate of Passenger Trains at Departure (%) | 99.8 | 99.7 | 99.8 | 99.5 | 99.8
Punctuality Rate of Passenger Trains in Running (%) | 97.6 | 96.5 | 95.9 | 98.4 | 99.4
Technical Speed of Passenger Trains (km/hr) | 71.4 | 71.7 | 73.7 | 74.2 | 74.7
Traveling Speed of Passenger Trains (km/hr) | 62.0 | 62.2 | 64.4 | 65.2 | 65.4
Density of Passenger Transport | 807.0 | 765.0 | 903.0 | 938.0 | 1002.0
(10 000 passenger-km/km) |  |  |  |  |
Technical Speed of Freight Trains (km/hr) | 47.1 | 47.1 | 46.7 | 46.3 | 46.2
Running Speed of Freight Trains (km/hr) | 32.4 | 32.8 | 32.2 | 32.1 | 32.1
Density of Freight Transport (10 000 ton-km/km) | 2533 | 2726 | 2997 | 3140 | 3242
Turning Around Time of Freight Cars (day) | 5.10 | 5.10 | 4.94 | 4.90 | 4.87
Handling Time of Freight (hour) | 21.2 | 20.9 | 17.2 | 15.2 | 15.2
Transfer Waiting Time per Car (hour) | 4.6 | 4.5 | 4.4 | 4.3 | 4.4
Static Load of Freight Cars (Standard Gauge) (ton) | 58.2 | 58.3 | 59.3 | 60.1 | 60.9
Utilization Rate of Loading Capacity of Freight Cars (%) | 96.7 | 96.5 | 98.0 | 98.7 | 99.2