Length of Railways in Operation refers to the total length of the trunk line under passenger and freight transportation (inc

Transport, Post and Telecommunication Services

Length of Railways in Operation refers to the total length of the trunk line under passenger and freight transportation (including both full operation and temporary operation). The calculation is based on the actual length of the first line even if this line has a full or partial double track or more tracks, excluding double tracks, station sidings, tracks under the charge of stations, branch lines, special-purpose lines and the non-payable connecting lines. The length of railways in operation is an important indicator to show the development of the infrastructure for the railway transport, and also the essential data to calculate volume of passenger freight transport, traffic density and utilization efficiency of the locomotives and carriages.

Extenuation Length of Trunk Lines refers to the sum of the first, the second, the third lines and other constructed length of the trunk railways, excluding the extenuation length of the station lines, lines under the jurisdiction of depots, sidings and lines for special purpose. It provides important information for the calculation of the needs for rails, sleepers, sand and stone for the construction of railways.

Length of Electrified Railways refers to the length of the section of railways in operation in which the power supply lines and other equipment are installed for the running of electrified locomotives. The proportion of the length of electrified railways to the total length of railways in operation is an important indicator to show the modernization of railways.

Automatic-blocking and Semi-automatic-blocking Length of Railways Blocking is a spacing technique by which a section of the railway only allows one train to pass at a time, in order to ensure the traffic safety. Automatic (semi-automatic) blocking length of railways refers to railways installed with equipment to perform automatic or manual blocking of trains, the proportion of automatic/semi-automatic blocking length to the total length of railways in operation is an important indicator to show the modernization of railways.

Length of Highways refers to the length of highways which are built in conformity with the grades specified by the highway engineering standard formulated by the Ministry of Communications, and have been formally checked and accepted by the departments of highways and put into use. The length of highways includes that of the suburb highways at large and medium-sized cities, highways passing through streets at small cities and towns, and also the length of bridges and ferries. It does not include the length of streets in big and medium-sized cities and highways built for the production purpose at factories, mines, forest areas and agricultural areas. If two or more highways go the same section of the way, the length of the section is only calculated for once and no duplication is allowed. The length of highways is an important indicator to show the development of the highway construction and to provide essential information to calculate the transport network density.

Length of Navigable Inland Waterways an indicator reflecting the size and development of inland water network, it refers to the length of the natural rivers, lakes, reservoirs, canals, and ditches open to navigation during a given period, which enables the transport by ships and rafts. It includes the channels open to navigation for over an accumulative 3 months in a year, yet this does not include the river courses which are only used to float odd logs and bamboo rafts.

Length of Civil Aviation Routes refers to the length of all routes for regular civil aviation flights. There are usually two ways to calculate the distance between airports connected by the route length: One is to put the length of all air routes together, called duplicated calculation of the length of the routes; the other is not to allow the duplication in calculation when two or more routes passing the same section of aviation routes. The latter is usually used, as it can precisely show the size of the civil aviation network and indicate the extent of civil aviation serving the national economy and the people.

Length of Oil (Gas) Pipelines used as an indicator to show the development, scale and level of the pipeline transportation, it refers to the actual transport distance of oil (or gas) products, and is in general calculated in the length of single pipe line. If the length of the double pipelines and alternate pipeline are included, it is called the extension length of the oil (gas) pipelines, which indicates the actual length of the pipelines built, excluding double pipelines.

Freight (Passenger) Traffic refers to the volume of freight (passenger) transported with various means. Freight transport is calculated in tons and passenger traffic is calculated in the number of persons. Despite the type of freight and travelling distance, the freight transport is calculated in the actual weight of the goods: and despite the travelling distance and ticket price, the passenger traffic is calculated by the principle that one person can be counted only once in one travel. The passenger who travel with a half price ticket or a child ticket is also calculated as one person. The freight (passenger) traffic provides a quantitative measure to show how the transport industry serves the national economy and people, and is also an important indicator for planning the transport industry and for studying the development scale and speed of the transport industry.

Freight (Passenger) Traffic Density refers to the freight (passenger) traffic volume carried by a particular means of transportation during a given period through one kilometer of a specific section of transportation route. The formula is as follows:

Freight (Passenger) Traffic Density=[Freight Ton-kilometers (Passenger-kilometers)] / (Length of Route in Operation)

Measuring unit: ton-kilometer / kilometer (or person-kilometer / kilometer)

Freight (passenger) traffic density reflects the degree of business of freight (passenger) traffic on transportation routes, and therefore provides important information for balancing transport capability, planning construction and upgrading of transport routes and studying the distribution of transport network.

Freight Ton-kilometers (Passenger-kilometers) refer to the sum of the products of the volume of transported cargo (passengers) multiplying by the transport distance, usually using ton-kilometer and passenger-kilometer as units for measurement. Normally, the shortest distance between the departure station and the destination station (i.e., the payable distance) is the basis to calculate the freight ton-kilometers. This is an important indicator to show the total results of the transport industry, to prepare and examine the transport plan and to measure the efficiency, the labour productivity and the unit cost of transport.

The formula is as follows:

Freight Ton-kilometers (Passenger-kilometers) =∑{Freight (Passenger) Traffic x Distance of Transportation}

Measuring unit: ton-kilometer (person-kilometer)

Static Load of Freight Cars refers to the average cargo weight as loaded by each freight car under the static condition at the departure station. It is used to show the utilization extent of the loading capacity of the freight cars. The formula is:

Static Load (ton) of Freight Car=(Tonnage of Goods Dispatched) / (Number of Freight Cars Loaded)

The static load of freight cars is determined by the nature and type of goods loaded, the type of vehicles, and the technique of loading. The difference between the average marked load and the static load of freight cars reflects the utilization of loading capacity of freight cars. For its calculation the following formula is applied:

Utilization Rate of Capacity of Freight Cars(%)=[(Average Static Load)×100%] / (Average Marked Load)

Average Daily Haul of Freight Locomotives refers to the average total ton-kilometers accomplished by each freight transport locomotive over day and night during a given period of time. It includes both the weight of the goods carried and the dead weight of the train itself. It is a comprehensive indicator reflecting the locomotive efficiency in terms of both time and the pulling force.

Average Daily Haul of Freight Transport Locomotive (ton-kilometer)=[(Total Ton/(Kilometers of Freight)] / (Daily Number of Freight Transport Locomotive)

Volume of Freight Handled in Major Coastal Ports refers to the volume of cargo passing in and out the harbor area of the major coastal ports and having been loaded and unloaded. The volume includes that of the postal matters, registered luggage and fuels, materials and fresh water as supplies of the ships. The volume of freight handled may be classified by direction of flow as freight for import and freight for export, or by nature of cargo as freight for domestic trade and freight for foreign trade. As an important indicator, the volume of freight handled by type of cargo and by main flow direction reflects the production capacity of ports.

Business Volume of Post and Telecommunications refers to the total amount of post and telecommunications services, expressed in value terms, provided by the post and telecommunications departments for the society. Post and telecommunication services can be classified as letters, parcels, remittance, issue of newspapers and magazines, fast mail service, express mail service, savings deposits, stamps for collection, public and individual telegraph service, facsimiles, long-distance telephone service, leasing of telephone lines, urban paging service, mobile telephone service, data transfer and transmission, etc. The accounting approach is to multiply the service products of all types with their average unit price (constant price) to get sum of business value, plus income from other services such as leasing of telephone lines and equipment, maintenance of telephone switchboards and lines on behalf of customers. This indicator reflects the overall results of post and telecommunications service during a given period, and is important to study the composition of business service and the development of post and telecommunications service.

The formula is as follows:

Business Volume of Post and Telecommunications=∑(Transaction of Post and Telecommunication Service x Constant Price) + Income from Leasing, Maintenance and other Services

Subscribers of Wireless Paging Services Wireless paging service refers the service by which telephone users send audio, digital or character signals to persons carrying small-size pagers within the designated areas through wireless paging centers. The page carriers who have registered in paging centers are counted as paging subscribers.

Mobile Telephone Subscribers refer to the persons who own mobile telephone numbers and are connected with the mobile telephone communication network through the mobile telephone switchboards. The number of subscribers is calculated by the subscribers who have completed registration at mobile communication business centers and entered into the mobile telephone network. One mobile telephone is taken as a subscriber.

Telephone Subscribers refer to subscribers that are connected to the public line telephone network provided with telephone services. Before 1997, telephone subscribers were classified as city subscribers and village subscribers. City subscribers referred to those connected to city telephone networks in county towns and cities, while village subscribers referred to those connected to village telephone stations at and below counties. Since 1997, the classification of telephone subscribers was modified on the basis of physical location of the subscribers as 搖rban telephone subscribers and 搑ural telephone subscribers, which is different from the previous classification of categorizing 搇ocal telephones and 搑ural telephones, while the definition of total subscribers and total number of telephones remain unchanged.

Urban Telephone Subscribers refer to subscribers telephone subscribers, located at municipalities, cities under the jurisdiction of province, cities at prefectural level, downtown and suburb of city at county level town and county towns (including country towns where county government located, and towns of county level according to the administrative organizational system), that are connected to the public line telephone network, including rural mineral area, forest area, military area.

Rural Telephone Subscribers refer to telephone subscribers, located at towns under county town and country, that are connected to the public line telephone network.

Household Telephone Subscribers refer to telephone sets installed in the dwelling units of urban or rural residents, and registered as residence subscribers for payment, including 3 types of payment for the service: private payment, public payment and free service.

Capacity of Office Telephone Exchanges refers to the capacity (measured in gate) of telephone exchanges installed in the offices of local telecommunication service providers for communication between fixed telephones. It includes the capacity of both manual and automatic exchanges in use and for stand-by purpose. Equipment with expansion function is to be counted by the expanded capacity.