o27e

15-27 PRINCIPAL ECONOMIC AND TECHNICAL INDICATORS OF RAILWAY TRANSPORTATION
Item | 1985 | 1996 | 1997 | 1998
Average Daily Ton-kilometers of Freight Locomotives (10 000 ton-km) | 93.1 | 93.0 | 94.5 | 94.5
Steam Locomotives | 55.2 | 53.9 | 50.5 | 44.3
Diesel Locomotives | 104.1 | 101.7 | 101.5 | 98.6
Electric Locomotives | 101.4 | 100.3 | 99.3 | 99.0
Average Total Tonnage of Freight Locomotives(ton) | 2597.0 | 2603.0 | 2632.0 | 2633.0
Steam Locomotives | 2000.0 | 1984.0 | 1936.0 | 1804.0
Diesel Locomotives | 2663.0 | 2632.0 | 2642.0 | 2604.0
Electric Locomotives | 2840.0 | 2865.0 | 2856.0 | 2861.0
Daily Distance per Freight Locomotive (km) | 424.0 | 422.0 | 428.0 | 430.0
Daily Distance per Passenger Locomotive (km) | 496.0 | 491.0 | 504.0 | 507.0
Coal Consumption of Steam Locomotives (kg/10 000 ton-km) | 137.4 | 141.9 | 155.6 | 175.8
Oil Consumption of Diesel Locomotives (kg/10 000 ton-km) | 24.2 | 24.6 | 25.2 | 26.0
Electricity Consumption of Electric Locomotives (kwh/10 000 ton-km) | 109.4 | 109.9 | 111.7 | 112.7
Punctuality Rate of Freight Trains at Departure | 95.2 | 95.2 | 95.5 | 96.0
Punctuality Rate of Freight Trains in Running | 94.4 | 94.6 | 94.6 | 96.0
Punctuality Rate of Passenger Trains at Departure | 99.3 | 99.4 | 99.3 | 99.6
Punctuality Rate of Passenger Trains in Running | 92.7 | 82.5 | 93.5 | 94.4
Technical Speed of Passenger Trains (km/hr) | 58.3 | 58.7 | 62.8 | 64.2
Travelling Speed of Passenger Trains (km/hr) | 49.0 | 49.5 | 53.3 | 54.5
Number of Coaches per Passenger Train (coach) | 16.1 | 16.2 | 16.2 | 15.8
Density of Passenger Trains (train/day) | 17.8 | 17.3 | 18.5 | 20.8
Density of Passenger Transportation (10 000 passenger-km/km) | 649.0 | 586.1 | 615.6 | 641.0
Number of Coaches per 10 000 Passengers(coach) | 0.32 | 0.32 | 0.32 | 0.31
Number of Coaches per 1 Million Passengers (coach) | 0.09 | 0.07 | 0.08 | 0.08
Technical Speed of Freight Trains (km/hr) | 44.3 | 44.1 | 45.3 | 45.8
Running Speed of Freight Trains (km/hr) | 30.2 | 30.4 | 31.4 | 31.8
Proportion of Through Freight Trains | 46.5 | 46.2 | 45.4 |
Density of Freight Trains (train/day) | 39.4 | 38.0 | 37.7 | 35.4
Density of Freight Transportation (10 000ton-km/km) | 2350.0 | 2279.9 | 2266.3 | 2129.4
Number of Cars per 10 000 Tons of Freight Traffic (car) | 2.7 | 2.7 | 2.7 | 2.9
Number of Freight Cars per 1 000 000 Ton-km (car) | 0.34 | 0.34 | 0.34 | 0.36
Turning Around Time of Freight Cars (day) | 4.50 | 4.48 | 4.57 | 5.48
Handling Time of Freight (hour) | 17.90 | 17.80 | 18.10 | 22.80
Transfer Waiting Time per Car (hour) | 4.50 | 4.60 | 4.60 | 5.20
Static Load of Freight Cars (Standard Gauge) (ton) | 56.80 | 57.20 | 57.30 | 57.60
Utilization Rate of Loading Capacity of Freight Cars | 97.60 | 98.30 | 96.50 | 96.60