16-25 Principal Economic and Technical Indicators of National Railway Transport
Item | 2001 | 2002 | 2003 | 2004 | 2005
Average Daily Ton-kilometers of Freight | 99.9 | 102.2 | 105.8 | 108.7 | 110.6
Locomotives (10 000 ton-km) |  |  |  |  |
Diesel Locomotives | 100.7 | 99.3 | 101.4 | 103.4 | 105.6
Electric Locomotives | 100.7 | 106.8 | 112.8 | 117.1 | 118.3
Average Total Tonnage of Freight Locomotives (ton) | 2760 | 2789 | 2829 | 2934 | 3038
Diesel Locomotives | 2668 | 2648 | 2679 | 2768 | 2848
Electric Locomotives | 2985 | 3028 | 3071 | 3198 | 3335
Daily Distance per Freight Locomotive (km) | 437 | 445 | 450 | 455 | 458
Daily Distance per Passenger Locomotive (km) | 533 | 557 | 562 | 612 | 650
Oil Consumption of Diesel Locomotives | 25.7 | 25.9 | 25.4 | 25.0 | 24.6
(kg/10 000 ton-km) |  |  |  |  |
Electricity Consumption of Electric Locomotives | 113.1 | 110.8 | 110.0 | 111.2 | 111.8
(kwh/10 000 ton-km) |  |  |  |  |
Punctuality Rate of Freight Trains at Departure (%) | 97.2 | 97.3 | 96.9 | 96.5 | 97.0
Punctuality Rate of Freight Trains in Running (%) | 96.8 | 96.7 | 96.5 | 96.2 | 96.9
Punctuality Rate of Passenger Trains at Departure (%) | 99.8 | 99.8 | 99.7 | 99.8 | 99.5
Punctuality Rate of Passenger Trains in Running (%) | 96.9 | 97.6 | 96.5 | 95.9 | 98.4
Technical Speed of Passenger Trains (km/hr) | 69.5 | 71.4 | 71.7 | 73.7 | 74.2
Traveling Speed of Passenger Trains (km/hr) | 60.5 | 62.0 | 62.2 | 64.4 | 65.2
Density of Passenger Transport | 785.0 | 807.0 | 765.0 | 903.0 | 938.0
(10 000 passenger-km/km) |  |  |  |  |
Technical Speed of Freight Trains (km/hr) | 46.7 | 47.1 | 47.1 | 46.7 | 46.3
Running Speed of Freight Trains (km/hr) | 39.5 | 32.4 | 32.8 | 32.2 | 32.1
Density of Freight Transport (10 000 ton-km/km) | 2412 | 2533 | 2726 | 2997 | 3140
Turning Around Time of Freight Cars (day) | 5.08 | 5.10 | 5.10 | 4.94 | 4.90
Handling Time of Freight (hour) | 22.0 | 21.2 | 20.9 | 17.2 | 15.2
Transfer Waiting Time per Car (hour) | 4.6 | 4.6 | 4.5 | 4.4 | 4.3
Static Load of Freight Cars (Standard Gauge) (ton) | 58.1 | 58.2 | 58.3 | 59.3 | 60.1
Utilization Rate of Loading Capacity of Freight Cars (%) | 97.3 | 96.7 | 96.5 | 98.0 | 98.7